{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":6,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Project File","C:\\temp\\sample",null,null,null,"If the temperature of a specific point exceeds the reference temperature, the analysis model is controlled so the the temperature does not rise further."]
["Reference Temperature [degree C]",100]
["Heat Source below Reference Temperature [W]",0.2]
["Heat Source above Reference Temperature [W]",0.05]
["Calculation Step [s]",0.1]
["Number of Calculation Steps",25]
["Controlling Coordinate (X[mm])",5]
["Controlling Coordinate (Y[mm])",3]
["Controlling Coordinate (Z[mm])",0.2]