{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["All Bodies (Temperature)","All Modes (Temperature)","All Bodies (loss density)","All Modes (loss density)","All Bodies (Elastic Strain) ","All Modes (Elastic Strain)"],"not_rendered":{"charts":0,"images":23,"macros":1,"external_links":0,"defined_names":0,"comments":6,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"All Bodies (Temperature)","index":0,"n_rows":10,"n_cols":7,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
["Calculation result file name (full path)","C:\\temp\\Ex7_en.pdt",null,"Setting item",null,null,"Heat Conduction Analysis Example 7"]
[null,null,null,"Retrieval result"]
[]
[]
[]
["mode number",0,"0 for static and steady analyses"]
[]
["Body ID","Body Attributes","Material Name","Integral Value","Average Value"]
[0,"VOL1","006_Glass_epoxy",1.744166709685632E-4,34.883334193712663]
[1,"VOL2","001_Alumina",4.9279563919565985E-5,61.599454899457527]

{"sheet":"All Modes (Temperature)","index":1,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["Calculation result file name (full path)","C:\\temp\\Ex8.pdt",null,"Setting item",null,"Heat Conduction Analysis Example 8"]
[null,null,null,"Retrieval result"]
[]
[]
[]
["Body ID",1]
[]
["mode number","Mode Label","Integral Value","Average Value"]
[0,"0.000000e+00[s]",2.0000000000000002E-5,25.000000000000021]
[1,"3.000000e+01[s]",2.5647860679244776E-5,32.05982584905599]
[2,"6.000000e+01[s]",2.9952060654117935E-5,37.440075817647447]
[3,"9.000000e+01[s]",3.3409576384395932E-5,41.761970480494945]
[4,"1.200000e+02[s]",3.6226252944123751E-5,45.282816180154718]
[5,"1.500000e+02[s]",3.8532567133162077E-5,48.16570891645263]
[6,"1.800000e+02[s]",4.0425771971550628E-5,50.532214964438325]
[7,"2.100000e+02[s]",4.1982259847273316E-5,52.477824809091679]
[8,"2.400000e+02[s]",4.3263253823352374E-5,54.079067279190504]
[9,"2.700000e+02[s]",4.4318305658540611E-5,55.397882073175801]
[10,"3.000000e+02[s]",4.5187752648737211E-5,56.484690810921556]
[11,"3.300000e+02[s]",4.5904553457792609E-5,57.380691822240806]
[12,"3.600000e+02[s]",4.6495706317926999E-5,58.119632897408792]
[13,"3.900000e+02[s]",4.6983366878817921E-5,58.72920859852244]
[14,"4.200000e+02[s]",4.7385740859836818E-5,59.232176074796065]
[15,"4.500000e+02[s]",4.77178031413583E-5,59.647253926697914]
[16,"4.800000e+02[s]",4.7991880560420189E-5,59.989850700525281]
[17,"5.100000e+02[s]",4.8218126277577125E-5,60.272657846971448]
[18,"5.400000e+02[s]",4.8404907094194733E-5,60.506133867743458]
[19,"5.700000e+02[s]",4.85591204276337E-5,60.698900534542169]
[20,"6.000000e+02[s]",4.8686454175472378E-5,60.858067719340518]

{"sheet":"All Bodies (loss density)","index":2,"n_rows":11,"n_cols":7,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Calculation result file name (full path)","C:\\temp\\ex11_en.pdt",null,"Setting item",null,null,"Electromagnetic wave analysis example 11 (Check option to calculate Q with high precision and set dielectric loss for DR)"]
[null,null,null,"Retrieval result"]
[]
[]
[]
["mode number",0,"0 for static and steady analyses"]
[]
["Body ID","Body Attributes","Material Name","Integral Value","Average Value"]
[0,"AIR","000_Air",0,0]
[1,"DR","DR_Mat",0.99988659494962806,3499849.3805341185]
[2,"AIR","000_Air",0,0]

{"sheet":"All Modes (loss density)","index":3,"n_rows":11,"n_cols":6,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["Calculation result file name (full path)","C:\\temp\\ex11_en.pdt",null,"Setting item",null,"Electromagnetic wave analysis example 11 (Check option to calculate Q with high precision and set dielectric loss for DR)"]
[null,null,null,"Retrieval result"]
[]
[]
[]
["Body ID",1]
[]
["mode number","Mode Label","Integral Value","Average Value"]
[0,"5.878961e+00GHz",0.99988659494962806,3499849.3805341185]
[1,"8.304711e+00GHz",0.99940770625511999,3498173.152140534]
[2,"8.304810e+00GHz",0.99937816015988357,3498069.7335292306]

{"sheet":"All Bodies (Elastic Strain) ","index":4,"n_rows":12,"n_cols":7,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Calculation result file name (full path)","C:\\Temp\\macro\\ex62_en_solid.pdt",null,"Setting item",null,null,"All Bodies (Equivalent Elastic Strain)"]
[null,null,null,"Retrieval result",null,null,"Stress Analysis Example 62 (Solid Body Model Results)"]
[]
[]
[]
["mode number",0,"0 for static and steady analyses"]
[]
["Body ID","Body Attributes","Material Name","Integral Value","Average Value"]
[0,"Substrate","001_Alumina",1.2687258665058281E-12,5.0749034660233164E-5]
[1,"Electrode1","008_Copper",7.4969666370402108E-13,1.4497014713039016E-3]
[2,"Electrode2","010_Nickel",1.1826426523221203E-13,9.1475866232479418E-4]
[3,"Electrode3","002_Gold",1.562704721912093E-13,1.2087317147053049E-3]

{"sheet":"All Modes (Elastic Strain)","index":5,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[]}
["Calculation result file name (full path)","C:\\Temp\\macro\\Ex6.pdt",null,"Setting item",null,"All Modes (Equivalent Elastic Strain)"]
[null,null,null,"Retrieval result",null,"Stress Analysis Example 6 (Deformation of Cantilever Beam Considering Large Deformation)"]
[]
[]
[]
["Body ID",0]
[]
["mode number","Mode Label","Integral Value","Average Value"]
[0," 0.05[Step]  ",6.1172005287163843E-2,7.6465006608954613E-4]
[1," 0.1[Step]  ",0.12248728607151679,1.5310910758939561E-3]
[2," 0.15[Step]  ",0.18405394942863776,2.3006743678579663E-3]
[3," 0.2[Step]  ",0.24598221752169022,3.0747777190211203E-3]
[4," 0.25[Step]  ",0.30838870026269793,3.8548587532837146E-3]
[5," 0.3[Step]  ",0.3713964540392512,4.642455675490628E-3]
[6," 0.35[Step]  ",0.43513738807222857,5.4392173509028438E-3]
[7," 0.4[Step]  ",0.49975454366510635,6.246931795813814E-3]
[8," 0.45[Step]  ",0.56540467604691591,7.0675584505864317E-3]
[9," 0.5[Step]  ",0.63226108379051094,7.9032635473813666E-3]
[10," 0.55[Step]  ",0.70051654017495224,8.7564567521868815E-3]
[11," 0.6[Step]  ",0.77038617119613906,9.6298271399517139E-3]
[12," 0.65[Step]  ",0.84211017407097555,1.0526377175887168E-2]
[13," 0.7[Step]  ",0.91595618555083902,1.144945231938546E-2]
[14," 0.75[Step]  ",0.99221915971915753,1.2402739496489438E-2]
[15," 0.8[Step]  ",1.0712122466932548,1.3390153083665651E-2]
[16," 0.85[Step]  ",1.153245314779366,1.4415566434742039E-2]
[17," 0.9[Step]  ",1.2385931116501365,1.5482413895626669E-2]
[18," 0.95[Step]  ",1.3275130776656905,1.6593913470821089E-2]
[19," 1[Step]  ",1.4205253055923739,1.7756566319904628E-2]