{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":6,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["プロジェクトファイル","C:\\temp\\sample",null,null,null,"ある位置の温度が基準温度を超えると制御されるサンプル"]
["基準温度[℃]",100]
["基準温度以下での発熱量[W]",0.2]
["基準温度以上での発熱量[W]",0.05]
["計算間隔[s]",0.1]
["計算ステップ数",25]
["制御点座標(X[mm])",5]
["制御点座標(Y[mm])",3]
["制御点座標(Z[mm])",0.2]