{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Area_BC","Area_ID","Volume_BA","Volume_ID"],"not_rendered":{"charts":0,"images":11,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Area_BC","index":0,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Full Path of Result File(.PDT) ","C:\\temp\\Ex7.pdt",null,null,null,"Contour Image of Watt Example No.7"]
["Boundary Condition Name","Minimum Value","Maximum Value",null,"Area[m2](In Range)",null,null,null,null,null,"BC2 is set to the top and bottom surfaces of the substrate"]
["BC2",0,30,null,2.9210937500000001E-3,null,null,null,null,null,"(Excluding Contact Surfaces with Heating Elements)"]
["BC2",30,100,null,1.6789062500000001E-3]
["BC2",0,100,null,4.5999999999999999E-3]
["BC1",0,61.5,null,7.5968424479166662E-5]
["BC1",61.5,100,null,3.2403157552083337E-4]
["BC1",0,100,null,3.9999999999999996E-4]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"BC1 is set to the top face of the heating element"]

{"sheet":"Area_ID","index":1,"n_rows":5,"n_cols":7,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["Full Path of Result File(.PDT) ","C:\\temp\\Ex7.pdt",null,null,null,null,"Contour Image of Watt Example No.7"]
["FaceID","BodyID","Minimum Value","Maximum Value",null,"Area[m2](In Range)"]
[1,0,0,30,null,1.4653645833333333E-3]
[5,0,0,30,null,1.4557291666666664E-3]
[7,1,61.5,100,null,3.2403157552083337E-4]

{"sheet":"Volume_BA","index":2,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
["Full Path of Result File(.PDT) ","C:\\temp\\Ex7.pdt",null,null,null,"Contour Image of Watt Example No.7"]
["Body Attribute Name","Minimum Value","Maximum Value",null,"Volume[m3](In Range)",null,null,null,null,null,"Tempearature of VOL1"]
["VOL1",0,30,null,2.8947061379750604E-6]
["VOL1",30,100,null,2.1052938620249438E-6]
["VOL1",0,100,null,4.9999999999999996E-6]
["VOL2",0,61.6,null,3.5177764892578121E-7]
["VOL2",61.6,100,null,4.4822235107421896E-7]
["VOL2",0,100,null,7.9999999999999943E-7]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Tempearature of VOL2"]

{"sheet":"Volume_ID","index":3,"n_rows":8,"n_cols":6,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Full Path of Result File(.PDT) ","C:\\temp\\Ex7.pdt",null,null,null,"Contour Image of Watt Example No.7"]
["BodyID","Minimum Value","Maximum Value",null,"Volume[m3](In Range)"]
[0,0,30,null,2.8947061379750604E-6]
[0,30,100,null,2.1052938620249438E-6]
[0,0,100,null,4.9999999999999996E-6]
[1,0,61.6,null,3.5177764892578121E-7]
[1,61.6,100,null,4.4822235107421896E-7]
[1,0,100,null,7.9999999999999943E-7]