{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["応力抽出マクロ","改訂履歴"],"not_rendered":{"charts":0,"images":5,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"応力抽出マクロ","index":0,"n_rows":14,"n_cols":11,"rows_kept":14,"cut":false,"hidden":false,"merged":[[2,3,2,5],[2,6,2,7],[3,9,9,9]]}
["計算結果ファイルのパス","C:\\temp\\Ex1.pdt"]
[]
[null,null,null,"抽出座標",null,null,"抽出結果"]
[null,null,null,"x座標","y座標","ｚ座標","最大主応力[Pa]","ミーゼス相当応力[Pa]",null,"使用方法\n・結果を抽出したい計算結果ファイルのフルパスを「計算結果ファイルのパス」欄に記入\n・格子座標空間の中心座標を「中心点**座標」欄に入力\n・格子座標空間の各軸±方向の間隔（単位は結果ファイルの解析単位に依存）、\nポイント数（中心点含まず）を「**軸±方向間隔」「**軸±方向ポイント数」欄に入力\n・計算結果抽出ボタンをクリック","Copyright© Murata Software Co., Ltd. All Rights Reserved"]
["中心点x座標",0.1,null,0.1,0,0.09,1207051.0764859384,693137.52362292807]
["中心点y座標",0]
["中心点z座標",0.09]
[]
["x軸±方向間隔",0.1]
["x軸±方向ポイント数",0]
["ｙ軸±方向間隔",0.1]
["y軸±方向ポイント数",0]
["ｚ軸±方向間隔",0.1]
["z軸±方向ポイント数",0]

{"sheet":"改訂履歴","index":1,"n_rows":4,"n_cols":5,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["更新履歴"]
["リリース日","バージョン","内容"]
["2020-04-01","V1.0","弊社サンプルマクロページに公開"]
[null,null,null,null,"Copyright© Murata Software Co., Ltd. All Rights Reserved"]